How to setup Novasina - iSens sensors
-------------------------------------

1) Connect USB connector -> Windows will setup an "USB Converter" (see device manager)
2) Open "USB Converter" settings -> Enable VLC (virtual serial port) -> Windows creates a new serial port
3) Enable GeckoR2 features -> FeatureSettings.xml
   - Instrument: iSens
   - Scanner: iSens
4) Check if the following dll's can be found in .\dll
   - ftd2xx.dll
   - iSens Novax Kommunikationsprofil.dll
   - NovaxComdll.dll
   - NovaxComDllWrp.dll
   - Utils.dll
5) Start GeckoR2 (with scanning enabled) -> In the part "Virtual Instrument" a Novasina iSens instrument with a serial number is shown

2018-06-18, Michael Russ