AmbientPressure=Ambient Pressure
DewPoint=Dew Point
ExternalOhms=External Ohms
ExternalTemp=External Temp
Flow=Flow
FrostPoint=Frost Point
HeadPressure=Head Pressure
HeadTemp=Head Temp
Lampvoltage=Lamp Voltage
MirrorOhms=Mirror Ohms
MirrorTemp=Mirror Temp
PPMv=PPMv
Photodiode=Photodiode
PreCoolerTemp=PreCooler Temp
RH=RH
RHw=RHw
CHAMBERPRESSURE=External Pressure
CTRLMODE=Control Mode
DEWPOINT=Dewpoint
DPSET=Dewpoint [SP]
ESDREASON=Error Code
EVPOS=Exp Valve Pos
EXPANSIONVALVETEMP=Exp Valve Temp
FLOWRATE=Flowrate
FLOWSET=Flowrate [SP]
FPSET=Frostpoint [SP]
FROSTPOINT=Frostpoint
FVPOS=Flow Valve Pos
LEVELPRESAT=Presat Level
PRESATTEMP=Presat Temp
REFRIGELOW=Refrige Low
REGULATEDPRESSURE=Regulated Pressure
RH1=Relative Humidity 1
RH1SET=Relative Humidity 1 [SP]
RH2=Relative Humidity 2
RH2SET=Relative Humidity 2 [SP]
RH3=Relative Humidity 3
RH3SET=Relative Humidity 3 [SP]
RUN=Run State
SATFLUIDTEMP=Saturator Temp
SATOUTTUBETEMP=Sat Out Temp
SATPRESSURE=Saturator Pressure
TEMP1=Temperature 1
TEMP2=Temperature 2
TEMP3=Temperature 3
TSSET=Saturator Temp [SP]
ControlModeDP=Dewpoint
ControlModeFP=Frostpoint
ControlModeRH1=RH 1
ControlModeRH2=RH 2
ControlModeRH3=RH 3
ILED=LED current
VPD=Photodiode
TLED=LED Temperature
LEDHTRPIDON=LED Heater On/Off
LEDHTRPIDSETPT=LED Heater Temp
TPD=PD Temperature
PDHTRPIDON=PD Heater On/Off
PDHTRPIDSETPT=PD Heater Temp
